#
# Shorewall version 4 - SIXXS Macro
#
# /usr/share/shorewall/macro.SixXS
#
#	This macro handles SixXS -- An IPv6 Deployment and Tunnel Broker
#
###############################################################################
#ACTION	SOURCE	DEST	PROTO	DEST	SOURCE	RATE	USER/
#				PORT(S)	PORT(S)	LIMIT	GROUP
#
# Used for retrieving the tunnel information (eg by AICCU)
PARAM	-	-	tcp	3874
#
# Used for signaling where the current IPv4 endpoint
# of the tunnel is and that it is alive
PARAM	-	-	udp	3740
#
# Used for tunneling IPv6 over IPv4 (static + heartbeat tunnels)
PARAM	-	-	41
#
# Used for tunneling IPv6 over IPv4 (AYIYA
# tunnels)(5072 is official port, 8374 is used in the beta)
PARAM	-	-	udp	5072,8374
#LAST LINE -- ADD YOUR ENTRIES BEFORE THIS ONE -- DO NOT REMOVE
