#!/bin/sh

RCDLINKS="2,S45 3,S45 6,K45"
################################################################################
#   Script to create a gre or ipip tunnel -- Shorewall 4
#
#   Modified - Steve Cowles 5/9/2000
#     Incorporated init {start|stop} syntax and iproute2 usage
#
#     This program is under GPL [http://www.gnu.org/licenses/old-licenses/gpl-2.0.txt]
#
#     (c) 2000,2001,2002,2003,2004,2005 - Tom Eastep (teastep@shorewall.net)
#
#   Modify the following variables to match your configuration
#
# chkconfig: 2345 26 89
# description: GRE/IP Tunnel
#
################################################################################

#
# Type of tunnel (gre or ipip)
#

tunnel_type=gre

# Name of the tunnel
#

tunnel="dfwbos"
#
# Address of your External Interface (only required for gre tunnels)
#
myrealip="x.x.x.x"

# Address of the local system -- this is the address of one of your
# local interfaces (or for a mobile host, the address that this system has
# when attached to the local network).
#

myip="192.168.1.254"

# Address of the Remote system -- this is the address of one of the
# remote system's local interfaces (or if the remote system is a mobile host,
# the address that it uses when attached to the local network).

hisip="192.168.9.1"

# Internet address of the Remote system
#

gateway="x.x.x.x"

# Remote sub-network -- if the remote system is a gateway for a
#                       private subnetwork that you wish to
#                       access, enter it here. If the remote
#                       system is a stand-alone/mobile host, leave this
#                       empty

subnet="192.168.9.0/24"

# GRE Key -- set this to a number or to a dotted quad if you want
#            a keyed GRE tunnel. You must specify a KEY if you
#            intend to load ip_conntrack_proto_gre on either
#            gateway system

key=

PATH=$PATH:/sbin:/usr/sbin:/usr/local/sbin

load_modules () {
    case $tunnel_type in
    ipip)
	echo "Loading IP-ENCAP Module"
	modprobe ipip
	;;
    gre)
        echo "Loading GRE Module"
        modprobe ip_gre
        ;;
    esac
}

do_stop() {

      if [ -n "`ip link show $tunnel 2>/dev/null`" ]; then
          echo "Stopping $tunnel"
          ip link set dev $tunnel down
      fi

      if [ -n "`ip addr show $tunnel 2>/dev/null`" ]; then
          echo "Deleting $tunnel"
          ip tunnel del $tunnel
      fi
}

do_start() {

      #NOTE: Comment out the next line if you have built gre/ipip into your kernel

      load_modules

      if [ -n "`ip link show $tunnel 2>/dev/null`" ]; then
          do_stop
      fi

      echo "Adding $tunnel"

      case $tunnel_type in
      gre)
          ip tunnel add $tunnel mode gre remote $gateway local $myrealip ttl 255 ${key:+key $key}
	  ;;
      *)
          ip tunnel add $tunnel mode ipip remote $gateway
	  ;;
      esac

      echo "Starting $tunnel"


      ip link set dev $tunnel up

      case $tunnel_type in
      gre)
          ip addr add $myip dev $tunnel
	  ;;
      *)
          ip addr add $myip peer $hisip dev $tunnel
	  ;;
      esac

      #
      # As with all interfaces, the 2.4 kernels will add the obvious host
      # route for this point-to-point interface
      #

      if [ -n "$subnet" ]; then
          echo "Adding Routes"
          case $tunnel_type in
          gre)
              ip route add $subnet dev $tunnel
	      ;;
	  ipip)
              ip route add $subnet via $gateway dev $tunnel onlink
              ;;
	  esac
      fi
}

case "$1" in
  start)
      do_start
    ;;
  stop)
      do_stop
    ;;
  restart)
      do_stop
      sleep 1
      do_start
    ;;
  *)
    echo "Usage: $0 {start|stop|restart}"
    exit 1
esac
exit 0
